

The new sbosdrv.sys driver is loaded from the config.sys file 
	and uses the untrasnd string as its parameter.

device=sbosdrv.sys ultrasnd=220,7,7,11,7

where 220 is the base port.
        7 is the P.C.M. interrupt.
       11 is the GF1 interrupt.

The user should remember to type SBOS at the DOS prompt to re-load the
	driver for any audio to be heard.

