GUS Daily Digest            Sat, 5 Mar 94 12:07 PST      Volume 11: Issue  30 

Today's Topics:
						 486/50 (non)Problem
						GUS & Doom on a 486-50
							   GUS0041
						GUS and ISA-bus speed
					   GUS Daily Digest V11 #28
				  GUS Daily Digest V11 #29 (2 msgs)
						   Megaem/QEMM7.03
						  MegaEm and QEMM 7
					   Noise on Output line...

Standard Info:
	- Meta-info about the GUS can be found at the end of the Digest.
	- Before you ask a question, please READ THE FAQ.

----------------------------------------------------------------------

Date: Fri, 4 Mar 1994 17:09:20 -0500 (EST)
From: Pete Kilcullen <pmk@access.digex.net>
Subject: Re: 486/50 (non)Problem

> A friend of mine has had trouble running Doom on his 486-50 Mhz, same goes
> for the games that use the 32-bit AIL drivers. What happens is that the
> machine resets and the GUS plays through all the samples that are loaded
> until ultrinit.exe is called again.

> Now, since it works fine on my 33-mhz and on his computer with a DX2-66
> we came to the conclusion that the GUS has trouble running Ultramid (if
> that indeed is what Doom uses; the shareware version did) on 50 mhz
> computers. Can this be so ? I have not seen this mentioned in the digest,
> and therefore find it a bit hard to swallow.

It is a bit hard to swallow. I've run aGUS card on my 486/50 for over a 
year. It works great with all GUS software, games, and DOOM! It must be 
another problem.

Pete

------------------------------

Date: Fri, 4 Mar 94 23:36:42 GMT+0200
From: Walter Prins <prins@itu1.sun.ac.za>
Subject: Re: GUS & Doom on a 486-50

>From: Broderdue <iqivar@hp1.cbs.dk>
>Subject: Doom on 486-50, Dune 3 and Origin

>A friend of mine has had trouble running Doom on his 486-50 Mhz, same goes
>for the games that use the 32-bit AIL drivers. What happens is that the
>machine resets and the GUS plays through all the samples that are loaded

>that indeed is what Doom uses; the shareware version did) on 50 mhz
>computers. Can this be so ? I have not seen this mentioned in the digest,
>and therefore find it a bit hard to swallow.
Well, I have a 486DX-50 with a very normal Tseng ET4000 
SVGA with 1 Meg, Seagate brand IDE controller,  GUS with 1Meg and a 
ISA bus running at 10Mhz (Clk/5) The motherboard is a Sis VLB board
with AMI bios on it.

Using this setup, Doom works fine. No problems whatsoever.
I don't think the problem lies with the 50Mhz chip.   Check the BIOS 
settings.  Perhaps the bus speed is too high or something (I'm guessing)

Ciao.

------------
Walter Prins                                  Email: prins@itu.sun.ac.za
Computer Science                                     prins@teppic.sun.ac.za
University of Stellenbosch, South Africa

------------------------------

Date: Fri, 4 Mar 94 15:09:06 CST
From: peticola%alpha@eagle.is.lmsc.lockheed.com (Dave Peticolas)
Subject: GUS0041

	A warning to anyone installing the gus0041?.zip upgrade:  If you have
Borland C++ 4.0 or any program which uses version 2 of the Borland custom controls
DLL file, the gus install program will overwrite the new version with an older one!
You should copy the file (BWCC.DLL) to another name, and then copy it back over.
I haven't checked to see if the GUS programs can use the new version yet, though.

Dave Peticolas

------------------------------

Date: Sat, 5 Mar 94 09:05:41 -0500
From: liaor@churchst.ccs.itd.umich.edu
Subject: GUS and ISA-bus speed

Hey, I ran my GUS in a 33MHz i486sx (ISA), with a bus speed of 1MHz
(clck/3) and I never had any problems.

Well, I always had problems with QEMM and certain games (like Dune 2, for
example) using SBOS or ULTRAMID, but MEGAEM escaped these problems.
I don't know if the bus speed had anything to do with it, but you never can
tell with the IBM's convoluted architecture.

Anyway, using EMM386 fixed my problems (so I had a separate config.sys file
for using EMM386 when worst came to worst.)  

Once in a while, wheN I played a MIDI file under Windows 3.1, I swear I could
tell a note dropped out.  But when I played that section of the MIDI file
again, I couldn't find any dropped note.  Was it justme?  Oh yeah, this was
with the "new" drivers (the ones that came with PMAKER)

------------------------------

Date: Fri, 4 Mar 1994 14:55:44 -0500 (EST)
From: Phat H Tran <ptran@sciborg.uwaterloo.ca>
Subject: Re: GUS Daily Digest V11 #28

> Date: Wed, 2 Mar 94 23:05:58 MET
> From: Broderdue <iqivar@hp1.cbs.dk>
> Subject: Doom on 486-50, Dune 3 and Origin
> 
> So, in order to track the problem down, we opened his computer and
> popped in a DX2-66 mhz, and everything worked without any problems at
> all. Furthermore, after placing his 50-mhz back in, we tried exchanging
> GUS cards (I have rev 3.4 of the card, he has rev 2.4), but the same
> problems re-appeared on his computer. It even worked fine with a DX2-50,
> and we tested his 50-mhz on another motherboard, but whoa, boom, schmack,
> the game still went down when running on the 50-mhz processor.
> 
> Now, since it works fine on my 33-mhz and on his computer with a DX2-66
> we came to the conclusion that the GUS has trouble running Ultramid (if
> that indeed is what Doom uses; the shareware version did) on 50 mhz
> computers. Can this be so ? I have not seen this mentioned in the digest,
> and therefore find it a bit hard to swallow.

I don't think the speed of the motherboard is to blame but probably some 
other peculiarity in the MB.  Both DOOM and the 32-bit AIL drivers run in
protected mode, so your friend might need to use the low IRQs (7 or lower) for
both the GF1 IRQ and the SB/MIDI IRQ.  Playing DOOM and certain games with the
32-bit AILs while my GUS is on IRQ 12 will cause intermittent crashes on my
machine.

DOOM doesn't use Ultramid.  Its GUS code is integrated into the game.  The
32-bit AIL's don't use Ultramid either.  You should unload Ultramid whenever
you want to play DOOM or a game that uses the 32-bit AILs.

> Date: Wed, 02 Mar 1994 12:28:54 GMT
> From: Clarke Brunt <CLARKE@lsl.co.uk>
> Subject: Re: gus0038 and gus0040
> 
> Secondly, the UltraSound setup part of install repeatedly
> told me that SoundBlaster DMA was failing on read, yet if I said to
> proceed regardless, I could then test the settings with NO failure.
> Does this matter? I haven't observed any REAL problems.

The new setup has been rather flaky for me.  It always fails the SBOS
and DMA diagnostics on my machine.

> Date: Wed, 2 Mar 94 19:20:22 PST
> From: "Simeon Ventura" <SVENTURA@BCSC02.GOV.BC.CA>
> Subject: Just bought a GUS
> 
> To: GUS     --INTERNET gus-general-owner@
> 
> 
> I just bought a GUS and am very happy with it. However, after playing
> around with it and the software that came with it and after reading the
> digests and the Usenet, I seem to be lacking Midisoft Recording Studio
> and Power Chords. I ftp'd the latest version of the disks down and the
> latest update disks, read the readmes, and found that those two apps
> are only available when you purchase the GUS. Well I purchased the GUS,
> so why don't I get those apps? Or, heaven forbid, do I have to shell out
> some more coin to get those fine apps?

What disks did your GUS come with?  If you have disks earlier than version 
2.06, then your GUS was packaged before Gravis were shipping Powerchords and
Session with their card.  Mailing in your registration card _should_ get
you those two apps.

> Date: Wed, 2 Mar 1994 10:35:08 -0700 (MST)
> From: re7813ke@meteor.uscolo.edu (Is this ship sinking?)
> Subject: Might and Magic w/ Megaem
> 
> Dear Gussers,
> 
>    I use Megaem to drive sound for might and magic 4 /5 World of Xeen, and
> when The intro for MM5 shows, there is alot of noise blocking large spots
> of voice.  It sound like interference you might get, putting your mouth
> too close to a microphone.  My setup is as follows:
> 
> 386dx25 (no bad chipsets)
> Ultrasound set on IRQ:7 DMA:1 MIRQ:11 ADDR:220
> Digiboard set on IRQ:5 no DMA
[...]
> 
> Anyone else have this problem?  Is it because of the IRQ:7 setting?

IRQ 7 does cause problems for digital audio on some machines, resulting in 
a lot of noise and other garbage to come out of your speakers.  Since IRQ 5
is already taken, try IRQ 3 or 4 for your MIDI/SB IRQ.  (4 is the IRQ for
COM1, and 3 is the IRQ for COM 2, so if you have a mouse on one of the com
ports, then choose the other IRQ.  COM port IRQs can usually be used by a
soundcard if the COM port isn't in use.)

> Date: Wed, 2 Mar 94 18:52:17 CST
> From: jhighto@squhs.uh.ilstu.edu (Josh Hightower)
> Subject: Patches...
> 
> Hi all,
>         I downloaded a the new gus0041a.zip & gus0041b.zip
> and I deleted the old ultrasnd directory.  Unfortunatly 
> all the patches weren't in the in two zip files.  So I 
> installed the patches came with the GUS.  But when I tried to  
> use install Megaem and then Emuset it told me the Charang.pat
> is missing.  I couldn't find where the patch is could someone
> out there tell me where I could find the patch.

Look on the 2.06L disks on the Epas mirrors.  If charang.pat isn't
on those, then try the file gus0034.zip.

> Date: Wed, 02 Mar 1994 12:36:13 GMT
> From: Clarke Brunt <CLARKE@lsl.co.uk>
> Subject: Re: PatchMaker
> 
> I notice that the PatchMaker help describes a button which is supposed
> to allow the part of the waveform after the loop section to be played
> on release (i.e. a sampled release), but the actual button does not
> seem to be present. Any comments?

The new Windows driver supports sampled release, so that feature was put
into a preliminary version of PML.  However, Bruce (PML's author) didn't
like how it turned out (a problem with the envelopes, I think) so he took 
out the support for sampled release.

> Date: Wed, 2 Mar 94 9:39:43 EST
> From: David Steinberg <desteinb@tews16.cs.hh.ab.com>
> Subject: Putt-Putt's Loud Music
> 
> I'm running the Putt Putt demos (for my kids, of course) and the
> volume levels of the music are very uneven. Sometimes the music
> gets so loud that the spoken words are drowned out. I've had this
> with both SBOS 3.7B2 and SBOS 3.81.

If the music volume is very uneven, then you might try configuring the
game for SB instead of Adlib (if it's currently configured for Adlib).

Phat.

------------------------------

Date: Sat, 05 Mar 94 18:42:27 +0200
From: Yossi Oren <LIOREN1@WEIZMANN.weizmann.ac.il>
Subject: Re: GUS Daily Digest V11 #29

>Date: Fri, 4 Mar 1994 12:46:13 -1
>From: KARL ERIK ASBJcRNSEN <KARLEA@stud.sarpih.no>
>Subject: .mtm multitracker
>
>I got down just1fix from epas. it was a .mtm-file. I took a look at
>it, and it said something about multitracker.
>Anyone know where to find it, or how to play .mtm's?
>
DMP 2.86 can play MTMs.
HTH,
Yossi.

+---+---+---+---------------------------------------------------+---+---+
| = | E |_|/|               Signature 1.2a                      | V | ^ |
+---+---+---+---------------------------------------------------+---+---+
|Yossi Oren, Al-Daf Techno-Mercenaries, Rishon Le-Zion, Israel. Help    |
++-----------------------------------------------++--------------------++
||Internet EMail:LIOREN1@WEIZMANN.WEIZMANN.AC.IL || The people are with||
||Bitnet EMail:LIOREN1@WEIZMANN                  ++ the Golan Heights! ||
|| "Even if you do live in this country, it doesn't mean  ++ DOOM!!    ||
||  you have to behave like an animal."           --Nati  || GUS!!     ||
+=========================================================++============+

------------------------------

Date: Sat, 05 Mar 94 18:45:40 +0200
From: Yossi Oren <LIOREN1@WEIZMANN.weizmann.ac.il>
Subject: Re: GUS Daily Digest V11 #29

>Date: Fri, 4 Mar 94 12:55:23 EST
>From: Rich Catena DTN 323-4371 <catena@arrcee.enet.dec.com>
>Subject: prob with some wav's in Encarta
>
>I'm having trouble with some of the wave files in ms encarta. Also the sounds
>on the intro screen don't sound. I think they are all the new ones added in
>94. THey are in the ...
>If i select one of these (for example John F. Kennedy's inaug. speech) i get
>an error dialog which says; " multimedia Wave MCI, no wave device that can
>play files in the current format is installed. Use drivers option to install
>wave device"

FTP to ftp.microsoft.com and get softlib/mslfiles/vfwrt1.exe (1.3MB).  It
includes a few codecs to get you going.
HTH,
Yossi.

+---+---+---+---------------------------------------------------+---+---+
| = | E |_|/|               Signature 1.2a                      | V | ^ |
+---+---+---+---------------------------------------------------+---+---+
|Yossi Oren, Al-Daf Techno-Mercenaries, Rishon Le-Zion, Israel. Help    |
++-----------------------------------------------++--------------------++
||Internet EMail:LIOREN1@WEIZMANN.WEIZMANN.AC.IL || The people are with||
||Bitnet EMail:LIOREN1@WEIZMANN                  ++ the Golan Heights! ||
|| "Even if you do live in this country, it doesn't mean  ++ DOOM!!    ||
||  you have to behave like an animal."           --Nati  || GUS!!     ||
+=========================================================++============+

------------------------------

Date: Fri, 4 Mar 1994 17:17:49 -0500 (EST)
From: Pete Kilcullen <pmk@access.digex.net>
Subject: Megaem/QEMM7.03

> Subject: Megaem & QEMM703
> 
> Hi! I have this problem I hope someone out there can help me with...
> 
> I have a 486 Dx2 66 Mhz Computer with one Gravis Ultrasound 1Mb installed.
> I have installed the QEMM386 v7.03 Memory manager on it. Everything works
> fine with the gus, both native and sbos support. But when I try to run
> megaem v2.02 (or any other version) I get the message that my EMS memory
> is not compatible. When I try to disable the EMS memory with the Megaem switchm
> I get a message telling me that the Gravis Ultrasound is currently in use
> buy another program.

There should be no conflict since I use both of these programs. Do you 
have QDPMI turned on and loaded when you load QEMM? Megaem is DPMI 
compliant.

Pete

------------------------------

Date: Sat, 5 Mar 1994 08:18:05 -0800 (PST)
From: mikebat@netcom.com (Mike Batchelor)
Subject: Re: MegaEm and QEMM 7

Not the GUS Server once wrote...
$  
$  ------------------------------
$  
$  Date: Wed, 2 Mar 94 21:25:32 +0100
$  From: svein harald fossum <fossum@nora.gih.no>
$  Subject: Megaem & QEMM703
$  
$  Hi! I have this problem I hope someone out there can help me with...
$  
$  I have a 486 Dx2 66 Mhz Computer with one Gravis Ultrasound 1Mb installed.
$  I have installed the QEMM386 v7.03 Memory manager on it. Everything works
$  fine with the gus, both native and sbos support. But when I try to run
$  megaem v2.02 (or any other version) I get the message that my EMS memory
$  is not compatible. When I try to disable the EMS memory with the Megaem switchm
$  I get a message telling me that the Gravis Ultrasound is currently in use
$  buy another program.
$  
$  The only problem is, there is no such program running.
$  
$  I forgot to mention that I have 4Mb of RAM. I ran the same program on my old machine.
$  That was a Copam 80486 Dx 25Mhz with 8Mb of RAM. On that machine everything worked
$  just fine.
$  
$  I would be most happy I someone could help me.

MegaEm works best of all with QEMM, as Jayeson will probably comfirm.  My
guess is that you have used up all 4Mb of memory before attempting to load
MegaEm.  It needs a 64K EMS handle.  If you are loading Smartdrv, that
might account for it, but a more likely culprit is PcKwik disk cache.  It
is supposed to share memory with other programs, but it fails to do so in
many cases.  It's default is to take over everything, and try to share
what it took.  Other caches will behave similarly, but PcKwik is the worst.

Other than that, I can only suggest that you load ONLY QEMM 7, and see if
it works then.  If it does, then one-by-one, add back in your other TSRs
and drivers until the cause is found.  I know it's not QEMM.

Oh, and do not use the EMS:N switch for QEMM, even if you use the
corresponding switch with MegaEm for -NOEMS.  The -NOEMS switch is risky
with any memory manager that has put the CPU in protected mode.

-- 
Mike Batchelor      | UseLinuxUseLinuxUseLinuxUseLinuxUseLinuxUseLinuxUseLinux
mikebat@netcom.com  | xuniLesUxuniLesUxuniLesUxuniLesUxuniLesUxuniLesUxuniLesU

------------------------------

Date: Fri, 4 Mar 1994 17:19:59 -0500 (EST)
From: fuller@hlsun.red-cross.org (Desmond Fuller)
Subject: Noise on Output line...

I've been a happy GUS users for almost 6 monthes now, but since I
updated to the new Window drivers I have had this annoying problem.

I have a set of Labtec CS-700 speakers and they turn on and off
when there is a signal.  When I am in DOS, they turn on and off
like there are suppose to.

Windows is another story.  When I first go into Windows and the
Startup noise plays they turn on but they fail to turn off.  They
click and the LED blinks (like they want to turn off but there is
noise on output channel).  If I go to the GUS mixer and MUTE LINE
OUTPUT and leave it for 10 seconds, the speakers turn off and 
everything is fine until I use the GUS again.

I have not added anything to my machine in monthes and I am at
a loss to explain this....

Any thoughts?

- Desmond

------------------------------

End of GUS Daily Digest V11 #30
*******************************
